




SECTION 13 34 16 - BLEACHERS
	GENERAL
	ADMINISTRATIVE REQUIREMENTS
	Pre-Installation Conference:
	Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder,] installer, and related trades.
	Review: Project conditions, manufacturer requirements, delivery and storage, staging and sequencing, and protection of completed work.
	SUBMITTALS
	Action Submittals:
	Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.
	Product Data: Manufacturer’s descriptive data and product attributes.
[bookmark: _Hlk37778578]	Samples: [Selection samples.] [Verification samples.]
	Informational Submittals:
	Certificate of Compliance: Certification that installed products meet specified design and performance requirements.
	Closeout Submittals:
	Maintenance Data.
[bookmark: _Hlk37778670]	QUALITY ASSURANCE
	Installer Qualifications:
	Firm specializing in work of this Section, with minimum [2] [__] years’ experience.
	Approved by bleacher manufacturer.
	Conform to [applicable accessibility code] [____] for access ramps and wheelchair spaces.
	SYSTEM DESCRIPTION
	Bleachers:
	Size: [15] [21] [27] feet long x [3] [4] [5] rows.
	Vertical rise: Maximum 6 inches per row.
	Horizontal depth: 21-3/4 inches per row.
	Seat height above tread: 16-3/4 inches.
	Aisle width: Minimum 48 inches.
	Design bleacher system to withstand following loads without damage or deformation of components:
	Live load: [100] [__] PSF on gross horizontal area; [120] [__] pounds per linear foot of seat and tread plank.
	Perpendicular sway load: [100] [__] pounds per linear foot of seat plank.
	Wind load: [30] [__] PSF on vertical projection.
	Guardrails: [100] [__] pounds per linear foot vertical; [50] [__] pounds per linear foot horizontal.
	Design system under direction of Professional Structural Engineer licensed in State in which Project is located, with minimum [2] [__] years [documented] experience in work of this Section.
	WARRANTY
	Manufacturer’s [3] [__] year warranty against defects in materials and workmanship.
	PRODUCTS
	MANUFACTURERS
A. Contract Documents are based on products by PW Athletic Manufacturing Co., Phone 866-402-2893; www.pwathletic.com.
B. Substitutions: [Refer to Division 01.] [Not permitted.]
	MATERIALS 
	Steel Shapes: ASTM A36/A36M.
	Aluminum:
	Extrusions: ASTM B221, 6061-T6 alloy and temper.
	Pipe: ASTM B241, extruded, anodizing quality, 6063 aluminum pipe, Schedule 40.
	Wood Mud Sills: Preservative treated for ground contact use.
	FABRICATION
	Shop assemble in largest practical units.
	Welding:
	Steel: AWS D1.1/D1.1M.
	Aluminum: AWS D1.2/D1.2M.
	Framework: Prefabricated [steel] [aluminum] angle type, with crossbracing.
	Risers: Extruded aluminum.
	Seats: Extruded aluminum, 1-1/2 inches high x 9-1/4 inches deep.
	Treads and Steps: Extruded aluminum planks with end caps.
	Guardrails: 
	Railings: 1.66 inch OD aluminum pipe with prefabricated fittings.
	Infill: [Galvanized steel chain link mesh.] [Vertical aluminum bars.]
	FINISHES
	Steel Frame: [Galvanized] [Manufacturer’s standard powder coat, sprayed and basked, [_____] color] ASTM A123/A123M, to 1.25 ounces per square foot.
***OR***

Aluminum Frame: [Mill Finish], [Manufacturer’s standard powder coat, sprayed and baked, [____] color.]

	Aluminum Planks: [Anodized coating, AAMA 607.1, to 0.0007 inch minimum thickness, [clear] [dark bronze.] [black.]] [Manufacturer’s standard powder coat, sprayed and baked, [____] color.]	Comment by ZeroDocs: Verify available finishes with bleacher manufacturer. Mill finish (unfinished) is the least expensive option and is often used where foot traffic could damage walking surfaces. Anodized and powder coated aluminum finishes also work well for non-walking surfaces.
	EXECUTION
	INSTALLATION
	Install in accordance with manufacturer's instructions and approved Shop Drawings.
	Installation Tolerances: 
	Variation from location: Plus or minus 1/2 inch.
	Variation from level or true plane: Maximum 1/4 inch in 10 feet.
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