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SECTION 07 46 49 – POLY-ASH SIDING
[bookmark: _heading=h.gjdgxs]POLY-ASH SIDING



SPECIFIER NOTE: THESE SPECIFICATIONS WERE CURRENT AT THE TIME OF PUBLICATION BUT ARE SUBJECT TO CHANGE AT ANY TIME WITHOUT NOTICE.  PLEASE CONFIRM THE ACCURACY OF THESE SPECIFICATIONS WITH THE MANUFACTURER AND/OR DISTRIBUTOR PRIOR TO CONSTRUCTION OR INSTALLATION.

GUIDE SPECIFICATIONS:
  
THIS GUIDE SPECIFICATION IS WRITTEN ACCORDING TO THE CONSTRUCTION SPECIFICATIONS INSTITUTE (CSI) FORMATS, INCLUDING MASTERFORMAT, SECTIONFORMAT, AND PAGEFORMAT.
 
CAREFULLY REVIEW AND EDIT THIS SECTION TO MEET THE REQUIREMENTS OF THE PROJECT, LOCAL BUILDING CODE AND AUTHORITIES HAVING JURISDICTION. COORDINATE THIS SECTION WITH OTHER SPECIFICATION SECTIONS AND DRAWINGS.

DELETE ALL "SPECIFIER NOTES" WHEN EDITING THIS SECTION.

PART 1 -  [bookmark: _heading=h.1fob9te]GENERAL
1.1  [bookmark: _heading=h.3znysh7]CONDITIONS AND REQUIREMENTS
A. [bookmark: _heading=h.2et92p0]The General Conditions, Supplementary Conditions, and Division 01 – General Requirements apply.
1.2  [bookmark: _heading=h.tyjcwt]SUMMARY 
A. Section Includes: 
1.  Poly-ash siding.
1.3  [bookmark: _heading=h.1t3h5sf]RELATED SECTIONS
[bookmark: _heading=h.2s8eyo1][bookmark: _Hlk79413631]*********************************************************************************************************************************************
SPECIFIER NOTES: ADD TO OR DELETE FROM THE FOLLOWING AS APPROPRIATE FOR THE SPECIFIC PROJECT.
*********************************************************************************************************************************************
A. Section 09 91 00 – Painting: Painting poly-ash siding with a topcoat.
1.4  REFERENCES
A. Reference Standards
*********************************************************************************************************************************************
SPECIFIER NOTES: RETAIN ONLY THOSE REFERENCES THAT ARE REQUIRED AFTER THE SECTION IS EDITED.
*********************************************************************************************************************************************
1.  American Society for Testing and Materials (ASTM):
a.  ASTM D570: Standard Test Method for Water Absorption of Plastics.  
b.  ASTM D1037: Standard Test Methods for Evaluating Properties of Wood-Base Fiber and Particle Panel Materials.
c.  ASTM D1622: Standard Test Method for Apparent Density of Rigid Cellular Plastics.
d.  ASTM D6109: Standard Test Methods for Flexural Properties of Unreinforced and Reinforced Plastic Lumber and Related Products.
e.  ASTM D6341: Standard Test Methods for Determination of the Linear Coefficient of Thermal Expansion of Plastic Lumber and Plastic Shapes between -30 and 140ºF.  
f.  ASTM E84: Standard Test Method for Surface Burning Characteristics of Building Materials.
2.  [bookmark: _heading=h.3as4poj][bookmark: _heading=h.3o7alnk]American Wood Protection Association (AWPA):
a.  [bookmark: _heading=h.3whwml4]AWPA E1: Laboratory Methods for Evaluating the Termite Resistance of Wood-Based Materials: Choice and No-Choice Tests.
b.  AWPA E10: Laboratory Method for Evaluating the Decay Resistance of Wood-Based Materials Against Pure Basidiomycete Cultures: Soil/Block Test. 
3.  California Department of Forestry and Fire Protection (CAL FIRE):
a.  Wildland-Urban Interface (WUI) CA SFM 12.7A-1 – Exterior Wall Siding and Sheathing.
1.5  SUBMITTALS
A. [bookmark: _heading=h.ihv636][bookmark: _heading=h.2grqrue][bookmark: _heading=h.3tbugp1]Comply with Section 01 33 00 – Submittal Procedures.
B. Product Data:
1.  Submit manufacturer's printed product literature, specifications, and data sheet.
C. [bookmark: _heading=h.32hioqz][bookmark: _heading=h.1hmsyys]Manufacturer’s Samples: Submit manufacturer’s sample of poly ash siding, minimum 6 inches by 6 inches. 
D. Certificates: Submit manufacturer’s certification that materials comply with specified requirements and are suitable for the intended application. 
E. Test Reports: Submit manufacturer’s test reports from testing performed by qualified, independent testing laboratories. 
F. Product Evaluation Reports: Submit manufacturer’s product evaluation reports from accredited evaluation services.
G. Warranty Documentation: Submit manufacturer’s standard warranty.
1.6  DELIVERY, STORAGE AND HANDLING
A. [bookmark: _heading=h.nmf14n][bookmark: _heading=h.111kx3o][bookmark: _heading=h.2zbgiuw]Storage and Handling Requirements:
1.  [bookmark: _heading=h.1mrcu09]Store and handle materials in accordance with manufacturer’s instructions. 
2.  Keep materials in protective covering until installation. 
3.  Store poly-ash siding covered and free of dirt and debris until installation.  
4.  Protect materials and finish during storage, handling, and installation to prevent damage.
1.7  WARRANTY
A. [bookmark: _heading=h.3ygebqi]Warranty Period for Poly-Ash Siding: 20 years.


PART 2 -  PRODUCTS
MANUFACTURERS
0. Specified Manufacturer: Westlake Royal Building Products, TruExterior® Siding & Trim Brand, 29797 Beck Rd, Wixom, MI 48393; 800-521-8486. Email: bianca.warner@westlake.net; Web: www.truexterior.com. 
*********************************************************************************************************************************************
SPECIFIER NOTES: DELETE ONE OF THE FOLLOWING TWO PARAGRAPHS.
*********************************************************************************************************************************************
Substitutions: Not Permitted.  
Requests for substitutions will be considered in accordance with provisions specified in Section 01 62 00 – Product Options.
POLY-ASH SIDING
Poly-Ash Siding: TruExterior® Siding:  
Shiplap siding used as exterior wall covering over sheathing on wood stud frame. 
Material: Polymeric blend, fly ash, and glass fibers.
Formed in continuous process, cut to 16-foot lengths, and milled to give a surface profile. 
Width: [5-1/2 inches (139.7 millimeters)], [7-1/2 inches (190.5 millimeters)], [9-1/2 inches (241.3 millimeters)], or [11-1/2 inches (292.1 millimeters)].  
Nominal Thickness: 3/4 inches (19.1 millimeters). 
*********************************************************************************************************************************************
SPECIFIER NOTES: SIDING CAN BE INSTALLED WITH EITHER SIDE EXPOSED TO ACHIEVE THE DESIGNED AESTHETIC.  THE SIDING IS INTENDED TO BE INSTALLED WITH THE FINISH/PROFILED SIZED AS THE EXPOSED SURFACE.
*********************************************************************************************************************************************
Exposed Texture: Smooth.  
Non-structural material. 
Listings and Reports:
Cal Fire (WUI), CA SFM 12.7A-1: Listing No. Listing No. 8140-2134:0103.
Product Evaluation Report: Progressive Engineering Inc., Evaluation Service, Report PER-13069.
Recycled Content: 
Post-Industrial Recycled Content: Minimum 70 percent, by weight. 
Post-Consumer Recycled Content: Minimum 2 percent, by weight.
Properties:
Density, ASTM D1622: 40 to 50 pounds per cubic foot (1.92 to 2.39 kilopascals).   
Flexural Strength, ASTM D6109: Greater than 1,600 pounds per square inch (11 032 kilopascals). 
Coefficient of Linear Expansion, ASTM D6341: Less than 1.40E-05 inch/inch/degree Fahrenheit (2.52E-05 millimeter/millimeter/degree Celsius).
Impact Resistance, ASTM D1037: Greater than 50 inches (1270 millimeters).
Performance:
Water Absorption, ASTM D570: Less than 1.5 percent. 
Fungi Rot: Conforming to AWPA E10: 
a.  White Rot: Negligible loss.  
b.  Brown Rot: Negligible loss.
Termite Resistance, AWPA E1: Greater than 9.0, with 10 being impervious.  
Surface Burning Characteristics:
c.  Flame Spread, ASTM E84: Between 25 and 29.
d.  Smoke Developed, ASTM E84: Less than 450.
FABRICATION: 
Manufacturing Tolerances: 
Width: Plus or minus 1/16 inches (1.6 millimeters). 
Thickness: Plus or minus 1/16 inches (1.6 millimeters).
Length: Plus 2 inches (50.8 millimeters), minus 0 inches. 
FINISHES
Primer: 
Acrylic based.  
Low volatile organic compound (VOC). 
Factory applied on all sides.
ACCESSORIES 
[bookmark: _heading=h.2r0uhxc]Fasteners:
Minimum 8d by 2-1/2 inches (63.5 millimeters) long stainless steel ring-shank nails.
In accordance with local building code.


1. [bookmark: _heading=h.3q5sasy]EXECUTION
3.1  EXAMINATION
A. [bookmark: _heading=h.25b2l0r]Examine wood framing members to receive poly-ash siding.
B. Notify Architect of conditions that would adversely affect installation or use.
C. Do not begin installation until unacceptable conditions are corrected.
3.2  INSTALLATION
A. Install poly-ash siding in accordance with manufacturer’s instructions at locations indicated on the Drawings.  
B. Poly-ash siding must not be installed in structural or load-bearing applications. 
C. Install poly-ash siding plumb, level, square, and true to line.  
D. Fasteners must be installed in accordance with local building codes.  
E. Painting:  
1.  Apply topcoat to poly-ash siding over factory-applied primer.  TruExterior® must be painted over the factory-applied primer or the warranty will be void.  
a.  Within 150 days of installing trim.  
b.  As specified in Section 09 91 00.  
F. Minor damages to poly-ash siding are to be repaired in accordance with manufacturer’s instructions and approved by Architect.  Damage that cannot be successfully repaired as determined by Architect must be removed and replaced with new material.
3.3  PROTECTION
A. Protect installed poly-ash siding to ensure that, except for normal weathering, trim will be without damage or deterioration at the of Substantial Completion.

[bookmark: _heading=h.xvir7l]END OF SECTION
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