

Header Info										Header Info
Header Info										Header Info
Header Info										Header Info
[image: ]

SECTION 06 65 00 – PLASTIC TRIM
[bookmark: _heading=h.gjdgxs]EXTERIOR SYNTHETIC TRIM

SPECIFIER NOTE: THESE SPECIFICATIONS WERE CURRENT AT THE TIME OF PUBLICATION BUT ARE SUBJECT TO CHANGE AT ANY TIME WITHOUT NOTICE.  PLEASE CONFIRM THE ACCURACY OF THESE SPECIFICATIONS WITH THE MANUFACTURER AND/OR DISTRIBUTOR PRIOR TO CONSTRUCTION OR INSTALLATION.

GUIDE SPECIFICATIONS:
  
THIS GUIDE SPECIFICATION IS WRITTEN ACCORDING TO THE CONSTRUCTION SPECIFICATIONS INSTITUTE (CSI) FORMATS, INCLUDING MASTERFORMAT, SECTIONFORMAT, AND PAGEFORMAT.
 
CAREFULLY REVIEW AND EDIT THIS SECTION TO MEET THE REQUIREMENTS OF THE PROJECT, LOCAL BUILDING CODE AND AUTHORITIES HAVING JURISDICTION. COORDINATE THIS SECTION WITH OTHER SPECIFICATION SECTIONS AND DRAWINGS.

DELETE ALL "SPECIFIER NOTES" WHEN EDITING THIS SECTION.

[bookmark: _heading=h.1fob9te]PART 1 - GENERAL
1.1  [bookmark: _heading=h.3znysh7]CONDITIONS AND REQUIREMENTS
A. [bookmark: _heading=h.2et92p0]The General Conditions, Supplementary Conditions, and Division 01 – General Requirements apply.
1.2  [bookmark: _heading=h.tyjcwt]SUMMARY 
A. Section Includes: 
1.  Exterior synthetic (poly-ash) trim.
1.3  [bookmark: _heading=h.1t3h5sf]RELATED SECTIONS
[bookmark: _Hlk79413631][bookmark: _Hlk79413659]*********************************************************************************************************************************************
SPECIFIER NOTES: ADD TO OR DELETE FROM THE FOLLOWING AS APPROPRIATE FOR THE SPECIFIC PROJECT.
[bookmark: _heading=h.4d34og8]*********************************************************************************************************************************************
A. [bookmark: _heading=h.2s8eyo1]Section 09 91 00 – Painting: Painting exterior synthetic trim.
1.4  [bookmark: _heading=h.17dp8vu][bookmark: _heading=h.lnxbz9][bookmark: _heading=h.44sinio][bookmark: _heading=h.1y810tw]REFERENCES
[bookmark: _Hlk79413678]*********************************************************************************************************************************************
SPECIFIER NOTES: RETAIN ONLY THOSE REFERENCES THAT ARE REQUIRED AFTER THE SECTION IS EDITED.
[bookmark: _heading=h.4i7ojhp]*********************************************************************************************************************************************
A. [bookmark: _heading=h.2xcytpi][bookmark: _heading=h.2bn6wsx]Reference Standards
1.  [bookmark: _Hlk79414048]American Society for Testing and Materials (ASTM):
a.  ASTM C1185: Standard Test Methods for Sampling and Testing Non-Asbestos Fiber-Cement Flat Sheet, Roofing and Siding Shingles, and Clapboards. 
b.  [bookmark: _Hlk79414122]ASTM D570: Standard Test Method for Water Absorption of Plastics. 
c.  ASTM D1761: Standard Test Methods for Mechanical Fasteners in Wood and Wood-Based Materials. 
d.  [bookmark: _Hlk79414140]ASTM D6341: Standard Test Methods for Determination of the Linear Coefficient of Thermal Expansion of Plastic Lumber and Plastic Shapes between -30 and 140ºF. 
e.  [bookmark: _Hlk79414149]ASTM E84: Standard Test Method for Surface Burning Characteristics of Building Materials.
2.  [bookmark: _Hlk79414389]American Wood Protection Association (AWPA):
a.  [bookmark: _heading=h.3whwml4]AWPA E1: Laboratory Methods for Evaluating the Termite Resistance of Wood-Based Materials: Choice and No-Choice Tests.
b.  AWPA E10: Laboratory Method for Evaluating the Decay Resistance of Wood-Based Materials Against Pure Basidiomycete Cultures: Soil/Block Test.
1.5  [bookmark: _heading=h.3as4poj][bookmark: _heading=h.3o7alnk]SUBMITTALS
A. [bookmark: _heading=h.ihv636][bookmark: _Hlk79414571]Comply with Section 01 33 00 – Submittal Procedures.
B. Product Data:
1.  Submit manufacturer's printed product literature, specifications, and data sheet.
C. [bookmark: _heading=h.32hioqz][bookmark: _heading=h.1hmsyys]Manufacturer’s Samples: Submit manufacturer’s sample of exterior synthetic trim, minimum 1 inch by 4 inches by 8 inches long (25.4 millimeters by 101.6 millimeters by 203.2 millimeters).  
D. Certificates: Submit manufacturer’s certification that materials comply with specified requirements and are suitable for the intended application.
E. Warranty Documentation: Submit manufacturer’s standard warranty.
1.6  [bookmark: _heading=h.2grqrue][bookmark: _heading=h.3tbugp1]DELIVERY, STORAGE AND HANDLING
A. [bookmark: _heading=h.nmf14n][bookmark: _Hlk79414740]Storage and Handling Requirements:
1.  [bookmark: _heading=h.1mrcu09]Store and handle materials in accordance with manufacturer’s instructions. 
2.  Keep materials in protective covering until installation. 
3.  Store exterior synthetic trim in a clean, dry area.  Exterior synthetic trim must be stored on a flat, level surface and be kept free of dirt and debris.  
4.  Protect materials and finish during storage, handling, and installation to prevent damage.
1.7  [bookmark: _heading=h.2lwamvv][bookmark: _heading=h.111kx3o][bookmark: _heading=h.2zbgiuw]WARRANTY
A. [bookmark: _heading=h.3ygebqi]Warranty Period for Exterior Synthetic Trim: 20-year limited warranty. 
1.  No decay due to rot.  
2.  No excel swelling from moisture.  
3.  Resists termite damage.


PART 2 -  [bookmark: _heading=h.sqyw64]PRODUCTS
MANUFACTURERS
[bookmark: _Hlk101867040]Specified Manufacturer: Westlake Royal Building Products, TruExterior® Siding & Trim Brand, 29797 Beck Rd, Wixom, MI 48393; 800-521-8486. Email: bianca.warner@westlake.net; Web: www.truexterior.com. 
*********************************************************************************************************************************************
SPECIFIER NOTES: DELETE ONE OF THE FOLLOWING TWO PARAGRAPHS.
*********************************************************************************************************************************************
Substitutions: Not Permitted.  
Requests for substitutions will be considered in accordance with provisions specified in Section 01 62 00 – Product Options.
EXTERIOR SYNTHETIC TRIM  
Exterior Synthetic (Poly-ash) Trim: TruExterior® Trim.  
Composition: 
Post-Industrial Recycled Content: Minimum 70 percent, by weight. 
Post-Consumer Recycled Content: Minimum 2 percent, by weight. 
Pigments and dyes.  
Physical Properties: 
Density, ASTM C1185: 40 to 50 pounds per cubic foot (1.92 to 2.39 kilopascals).  
Water Absorption, ASTM D570: Less than 1.5 percent. 
Fungi Rot: Conforming to AWPA E10: 
a.  White Rot: Negligible loss.  
b.  Brown Rot: Negligible loss.
Termite Resistance, AWPA E1: Greater than 9.0, with 10 being impervious. 
Mechanical Properties: 
Flexural Strength, ASTM C1185: Greater than 1,600 pounds per square inch (11 032 kilopascals).
Nail Withdrawal, ASTM D1761: Greater than 40 pound force inch (4.5 newton-meter).
Thermal Properties: 
Coefficient of Linear Expansion, ASTM D6341, Typical: 1.40E-05 inch/inch/degree Fahrenheit (2.52E-05 millimeter/millimeter/degree Celsius), tested at minus 30 to 140 degrees Fahrenheit (-34.4 and 60 degrees Celsius).
Flame Spread, ASTM E84: Between 25 and 29.
Smoke Developed, ASTM E84: Less than 450.
Trim Sizes: 
Trim Sizes: 
[bookmark: _Hlk79399729]*********************************************************************************************************************************************
SPECIFIER NOTES: TRIM SIZES TO BE SPECIFIED ON DRAWINGS.  CONSULT WESTLAKE ROYAL BUILDING PRODUCTS FOR AVAILABILITY OF TRIM SIZES.
*********************************************************************************************************************************************
c.  Nominal Size: 1 inch by 4 inches (25.4 millimeters by 101.6 millimeters).  Actual Size: 3/4 inches by 3-1/2 inches (19.1 millimeters by 88.9 millimeters). 
d.  [bookmark: _Hlk79399232]Nominal Size: 1 inch by 6 inches (25.4 millimeters by 152.4 millimeters).  Actual Size: 3/4 inches by 5-1/2 inches (19.1 millimeters by 139.7 millimeters).
e.  Nominal Size: 1 inch by 8 inches (25.4 millimeters by 203.2 millimeters).  Actual Size: 3/4 inches by 7-1/4 inches (19.1 millimeters by 184.2 millimeters).
f.  Nominal Size: 1 inch by 10 inches (25.4 millimeters by 254 millimeters).  Actual Size: 3/4 inches by 9-1/4 inches (19.1 millimeters by 235 millimeters).
g.  Nominal Size: 1 inch by 12 inches (25.4 millimeters by 304.8 millimeters).  Actual Size: 3/4 inches by 11-1/4 inches (19.1 millimeters by 285.5 millimeters).
h.  Nominal Size: 5/4 inches by 4 inches (31.75 millimeters by 101.6 millimeters).  Actual Size: 1 inch by 3-1/2 inches (25.4 millimeters by 88.9 millimeters).
i.  Nominal Size: 5/4 inches by 6 inches (31.75 millimeters by 152.4 millimeters).  Actual Size: 1 inch by 5-1/2 inches (25.4 millimeters by 139.7 millimeters).
j.  Nominal Size: 5/4 inches by 8 inches (31.75 millimeters by 203.2 millimeters).  Actual Size: 1 inch by 7-1/4 inches (25.4 millimeters by 184.2 millimeters).
k.  Nominal Size: 5/4 inches by 10 inches (31.75 millimeters by 254 millimeters).  Actual Size: 1 inch by 9-1/4 inches (25.4 millimeters by 235 millimeters).
l.  Nominal Size: 5/4 inches by 12 inches (31.75 millimeters by 304.8 millimeters).  Actual Size: 1 inch by 11-1/4 inches (25.4 millimeters by 285.5 millimeters).
m.  Nominal Size: 5/4 inches by 6 inches Beadboard (31.75 millimeters by 152.4 millimeters).  Actual Size: 5/8 inches by 5-1/4 inches (15.9 millimeters by 133.4 millimeters).
*********************************************************************************************************************************************
SPECIFIER NOTES: TRIM IS REVERSIBLE.  SPECIFY EXPOSED TEXTURE.
*********************************************************************************************************************************************
Exposed Texture: [Woodgrain] or [Smooth].
FABRICATION
Manufacturing Tolerances: 
[bookmark: _Hlk79664870]Width: Plus or minus 1/16 inches (1.6 millimeters). 
Thickness: Plus or minus 1/16 inches (1.6 millimeters).
Length: Plus 2 inches (50.8 millimeters), minus 0 inches. 
Edge Cut: Plus or Minus 2 degrees.

FINISHES
Primer: 
Acrylic based.  
Low volatile organic compound (VOC). 
Factory applied on all sides.
FASTENERS 
[bookmark: _heading=h.2r0uhxc]Specify minimum 16 gauge fasteners with head and finish suitable for the project environment and specific application.  Fasteners should be installed with adequate penetration to hold solid substrate.
Type: [Nails], [Screws], or [as indicated on the Drawings].
Size: [ _____] or [as indicated on the Drawings]. 
Finish: [Galvanized], [Stainless steel], or [as indicated on the Drawings].


1. [bookmark: _heading=h.3q5sasy]EXECUTION
3.1  EXAMINATION
A. [bookmark: _heading=h.25b2l0r]Examine surfaces to receive exterior synthetic trim.
B. Notify Architect of conditions that would adversely affect installation or use.
C. Do not begin installation until unacceptable conditions are corrected.
3.2  INSTALLATION
A. [bookmark: _heading=h.34g0dwd]Install exterior synthetic trim in accordance with manufacturer’s instructions at locations indicated on the Drawings.  
B. Exterior synthetic trim must not be installed in structural or load-bearing applications. 
C. Install exterior synthetic trim plumb, level, square, and with flush, tight joints.  
D. Fasteners must be installed a maximum of 24 inches (609.6 millimeters) on center and within 2 inches (50.8 millimeters) of the end of boards.  
E. Nail and screw holes are to be filled with acrylic caulk, wood filler, or autobody filler.  
F. Minor damages to exterior synthetic trim are to be repaired in accordance with manufacturer’s instructions and approved by Architect.  Damage that cannot be successfully repaired as determined by Architect must be removed and replaced.
G. Painting:  
1.  Apply topcoat to exterior synthetic trim over factory-applied primer. TruExterior® Trim must be painted over the factory-applied primer or the warranty will be void.  
a.  Within 150 days of installing trim.  
b.  As specified in Section 09 91 00.
3.3  PROTECTION
A. Protect installed exterior synthetic trim to ensure that, except for normal weathering, trim will be without damage or deterioration at the of Substantial Completion.

[bookmark: _heading=h.xvir7l]END OF SECTION
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